LT - 4 bar

LF.          725

RF.          775

LR.          725

RR.         750

2 inch set up blocks

LF. 3 turns in

RF. Touch

LR. 3 turns in

RR. Touch

Make race ready sit on shop floor with driver in

Ride height blocks

RR.   4 1/4

LR.   3 1/8

Add or subtract turns to get blocks to fit like a feller gage

If you have to go more than 5 turns in left rear than in RR bar go up a bar size

Front to be 1/2 higher than rear

If you have scales start in the 44 to 46% cross range