SUZUKI – 06 – 12 – 32 PLATE SET(new cars)

6 5/8 C/S HEIGHT

**SPACERS AND LOCATION**

 **F1 LOC**

RIGHT FRONT - NONE 10MM X 1.25 X 1 ¾ LONG BOLT

TOP LEFT NONE

LOWER LEFT .375 D2 A-11

TOP RIGHT 1.565 D2 C-5

LOWER RIGHT 1.590 D2 C-7

YOU WILL HAVE TO PUT( 2) .375 SPACERS ON THE OUTSIDE OF THE MOTOR D1 – A4

TUBES ( LEFT SIDE )

SHIFTER SHAFT MX7 - LATER - -020

SHIFTER ROD MOTOR 1 ¾ LONG

 HANDLE 3”

PLATE SET 32 -

RIGHT FRONT MOTOR MOUNT LOCATION BOTTOM 3 HOLES

PLATE SET – 26 RIGHT FRONT USES MIDDLE 3 HOLE

4/23/13 JM